# System Update Instructions for the Artis v1.10

updated 10/29/13

## FILES INCLUDED IN THIS DOWNLOAD:

Filename | Purpose
--- | ---
Artis-v110-OS Install Procedure.html | This document, detailing installation steps
Artis-v110-OS Release Notes.html | A detailed history of all OS enhancements and fixes
ARTSV110.KUF | Update file containing OS 2.26.1210, Objects 1.10.7 and Boot Loader 1.01.21288

## UPDATE METHODS:

The Artis can be updated by one of two methods:

- Method (a): USB storage device
  requires: Computer (Mac or PC) with USB port + USB Storage device - such as a flash/thumb drive (drives drawing 100 mA or less are recommended).
- Method (b):direct USB connection to computer
  requires: Computer (Mac or PC) with USB port + USB cable.

## UPDATE PROCEDURE:

### !! Before updating, be sure to back up any custom programming!! If unfamiliar with the process, please see the following links (or your manual) for details: "Saving User Data (USB Flash/Thumb Drive)" OR "Saving User Data (USB to Computer)."

1. Choose Update Method:

   (a) If updating via USB storage device (for ex. thumb drive) insert the device into to a free USB port on your computer.

   -OR-

   (b) If updating via USB-to-Computer connection, connect a USB cable between the Artis "Computer" USB port and any available USB port on your PC/Mac.

2. Enter SYSTEM MODE:

   Power the Artis OFF. Press/Hold the ENTER button and turn the Artis on. Release the ENTER button when the System Mode's menu of options appear on the screen:

       Artis System Mode         v1.01.21288 L2

       Run     System Run   System System
       Artis   Update Diags Reset  Utilities

   You will use the various "soft buttons" under the screen to control the update process.

3. Copy the Update File (.KUF):

(a) If updating via USB storage device: copy the included .KUF to the flash/thumb device using the method specific to your computer system. Once copied, safely eject/unmount the device before physically unplugging it from the computer's USB port. Once safely ejected, connect the device to the Artis "Storage" USB port.

(b) If updating via USB-to-Computer connection: at step 5 (below), when selecting "PC USB" as your update method, an Artis temporary "drive" will appear on your computer as a removable disk. At that time you will be instructed to copy (drag and drop) the .KUF update file to this temporary removable disk. Be sure to copy the ONE appropriate file when prompted. For now, proceed.

4. Press System Update:

       Artis System Mode         v1.01.21288 L2

       Run     System Run   System System
       Artis   Update Diags Reset  Utilities

5. Select Storage Type:

   Pick either-
   (a) USB Device (if installing from USB flash/thumb drive)
   -or-
   (b) PC USB** (if installing via direct USB-PC connection)

       Storage

       		USB    PC
       		Device USB         Back

   ** If choosing "PC USB" you will see a prompt on the Artis to copy the file now. On your computer, copy the .KUF update file to the temporary removable disk mounted on your computer. Once copied, safely eject the temporary removable disk from your computer, then press OK on the Artis to proceed.

       Copy File

       Copy file to Artis drive on your computer
       desktop. If already copied just press OK.

                                   OK     CANCEL

6. Use the data wheel, UP and OK buttons to navigate to and select the .KUF file (asterisk ∗ placed next to selection):

       Select File (.KUF files only) \
       * ARTSV110.KUF      4923K

       		     UP     OK     CANCEL

7. Press OK:

       Select File (.KUF files only) \
       * ARTSV110.KUF      4923K

       		     UP     OK     CANCEL

   A progress screen appears while the file is loaded.

       Installing
       Installing ARTSV110.KUF

           Extracting OS File

       			            80%

       		                   CANCEL

8. Press OK when complete:

       Installed

       File ARTSV110.KUF was installed.

       		                   OK

9. Power the Artis off and back on:

   The Artis will reboot to normal operating mode and is ready for use.

10. Confirm the OS and Objects were installed correctly: Once powered back up, go to GLOBAL mode, press the INFO menu soft button. Confirm you see the following:

        GlobalMode : SYSTEM INFO
        OS Version           :2.26.1210
        Object Version       :1.10.7

        MASTER MIDI   INFO   LOAD   STORE  RESET

    If for some reason the install did not complete properly, simply power off and repeat from the beginning (step 2).