# Kurzweil SP4 Series OS V2.00 Update

6/16/11

Past Release Notes

## OS Version 2.00 Release Notes

> CAUTIONS:

> Content created with v2.00 is not backwards compatible to older software versions. Content created with a SP4 older than v2.00 is of course forward compatible with 2.00.

> SETUP MODE:

> > Features:

> > - New: Delete option added under the Save dialog.

> > Fixes/Improvements:

> > - Fixed: program insert effects were sometimes not being loaded when selected in Edit Setup mode.
> > - Fixed: MIDI Bank value range extended.
> > - Fixed: Setup Edit Aux Send Level now can be edited to -1 (P).
> > - Fixed: Split and Layer showing the proper Setup Id when saving.
> > - Fixed: Save LED now on when accessing Split or Layer.
> > - Improved: smoother pitch wheel transition between setups.
> > - Fixed: several problems in pitch wheel setup process when pitch wheel settings were not defaults (linear curve, 100% scale and 0 add).
> > - Fixed: Local Keyboard Channel now working properly for remotely selecting setups.
> > - Fixed: problem selecting Setups that were empty.

> PROGRAM MODE:

> > Features:

> > - New: Delete option added under the Save dialog.

> EFFECTS:

> > Fixes/Improvements:

> > - Fixed: bug affecting FX in split/layer mode.

> GLOBAL MODE:

> > Features:

> > - New Load method: "Load [fill]?" - for use when loading PC3/LE/K series programs - loaded programs fill the User bank sequentially starting from the lowest available ID on upward, skipping any occupied locations.

> >   Note: Only one file may be loaded at a time. The file may itself contain multiple programs. To load more than one file, separate "Load [fill]?" operations must be performed.

> > - Name change: "Load All?" renamed "Load [overwrite?]" - this function is used for loading back in memory backups (.SPX files) created using the "Save All?" function. Performing a "Load [overwrite?]" erases the User bank replacing its contents with that of the loaded file.

> > Fixes/Improvements:

> > - Greatly improved ease of importing PC3/LE/K series programs. Previously several steps were required to get things to work. Now it is a straightforward procedure using the newly added "Load [fill]?" function (see above).
> > - Improved the translation accuracy of imported PC3/LE/K series programs.
> > - Fixed: a bug where manually ejecting the desktop PC/USB-Drive could make the drive unavailable and require a power cycle to regain access.
> > - Fixed: "Resetting" message now displayed while doing a hard reset.
> > - Improved handling of Global parameters saved across power cycles:

> >   The parameters that are remembered now are: - Category favorites - Velocity Map (Touch) - Local keyboard channel (LclKbdChan) - Program change (ProgChg) - Bank select (BankSel) - Destination (Dest) - Channel 1-16 enable (Chan#) - FX select (FXSel) - Sysex ID (SysexID)

> GENERAL:

> > Fixes/Improvements:

> > - Fixed: bugs leading to potential system freezes on power up.
> > - Fixed: previously, during bootup, MIDI coming in or plugging in a MIDI cable would freeze the unit.
> > - Fixed bug with USB MIDI that, under particular circumstances, could cause a noticeable delay in playing the keyboard while being connected to a computer via USB.
> > - Fixed: under particular circumstances the unit was not getting detected as a USB-MIDI device.
> > - Fixed: very rare occurrence of "missed pedal events".
> > - Fixed: stuck note bug where Note Offs were ignored when the keyboard was suddenly used to select a key (for eg. when choosing a split key)
> > - Fixed: was crashing when a MIDI connected PC3 was powered on.
> > - Fixed: demo was starting in response to MIDI start.

## Past Release Notes

### OS Version 1.10

> Initial Release

-END-